1. Active pedestrian spotted ahead
2. Distance between vehicles should be maintained during the traffic stop
3. If the number of vehicles is more than 20, send traffic space full information to other vehicles approaching so that they slow down
4. send alternate route suggestions to approaching vehicles
5. near a school zone (during peak hours)
6. Hospital zone
7. traffic ahead is high
8. accident has occurred
9. roadblock ahead (due to construction/police investigation)
10. Safe to take a turn or not should be requested and confirmed by



1. Sudden break by vehicle in the same lane out of sight
2. Nearby parking spots availability should be sent to the driver when requested
3. Emergency vehicles
4. Send information to traffic lights to prioritize that area
5. Clear the way for the emergency vehicle
6. Traffic light management (time) based on the number of vehicles
7. When fuel is less than the threshold, the nearest gas station is suggested. Next alternate Charging or gas stations are suggested when the number of vehicles present in a particular station is 2\*the number of outlets